|  |  |
| --- | --- |
| Portable electrospinning    PE95-1 | FEATURES:   * **Portable** * **working at most usual places** * **Ability to use as only syringe pump or only Electrospinning** * **0 – 30 KV DC power supply** * **High voltage protection** * **0.01 cc/h Minimum speed** * **900 cc/h Maximum speed** * **Glasses and plastics syringes** * **Syringes volume from 1cc to 20cc** * **Ultrasonic distance meter (3cm to 100cm )** * **Easy keypad interface** * **Programmable** * **Characteristic LCD** * **Ending Buzzer warning** * **220 v , 50 Hz input**   **Science-based company:**  **ZIST RAHE DANESH** |